{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":64,"n_cols":11,"rows_kept":64,"merged":[[0,0,0,10],[1,0,1,1],[2,0,17,1],[2,2,17,2],[2,10,17,10],[18,0,18,6],[19,0,29,1],[19,2,29,2],[19,10,29,10],[30,0,30,5],[31,0,51,1],[31,2,51,2],[31,10,51,10],[52,0,52,6],[53,0,61,1],[53,2,61,2],[53,10,61,10],[62,0,62,5],[63,0,63,6],[63,7,63,10]],"flags":["formulas_cached_only"]}
["安全工程系2016年度建筑实训室各工种物品采购清单"]
["实验室名称",null,"实验室\n面积/m2","设备名称","型号","价格（元）","数量","总计价格","技术参数","产  地","主要用途"]
["砌筑工操作实训室",null,100,"瓦刀","中号",null,24,{"$nulls":3},"砌筑工操作实训室是对学生进行砌筑工操作技能训练的教学场所。使学生通过实训认识常用砌筑施工机械与工具的功能并能进行简单使用，学生通过实训认识常用砌体材料、砂浆材料和其它辅助材料的种类与性能。\n帮助学生初步掌握砌筑工操作基本技能。主要完成简易砖墙、砖柱、砖基础的组砌，并通过各种组砌和摆砖，使学生懂得构成砌体的方法。\n"]
[{"$nulls":3},"泥桶","中号",null,24]
[{"$nulls":3},"线坠",null,null,8]
[{"$nulls":3},"托线板",null,null,8]
[{"$nulls":3},"皮数杆","2m",null,8]
[{"$nulls":3},"百格网",null,null,8]
[{"$nulls":3},"溜子","长号",null,8]
[{"$nulls":3},"托灰板",null,null,16]
[{"$nulls":3},"塞尺",null,null,8]
[{"$nulls":3},"钢卷尺","5m",null,9]
[{"$nulls":3},"砂浆搅拌机","200L",null,1]
[{"$nulls":3},"平头铁铲","中号",null,12]
[{"$nulls":3},"扫把",null,null,12]
[{"$nulls":3},"水管","透明牛筋软水管内径10mm,长60米",null,2]
[{"$nulls":3},"筛子","3mm",null,1]
[{"$nulls":3},"台秤","机械型",null,1]
["合计"]
["钢筋工操作实训室",null,200,"钢筋工台桌",null,null,13,{"$nulls":3},"钢筋工操作实训室是让学生进行练习钢筋弯制和绑扎的教学场所。使学生通过实训掌握钢筋工常用的设备、工具的使用和保管方法。帮助学生初步掌握钢筋工操作的基本技能。"]
[{"$nulls":3},"断丝钳","1050型",null,4]
[{"$nulls":3},"手摇扳",null,null,25]
[{"$nulls":3},"钢筋扳手","8mm",null,25]
[{"$nulls":3},"钢筋扳手","12mm ",null,25]
[{"$nulls":3},"钢卷尺","5m",null,25]
[{"$nulls":3},"扎丝钩",null,null,25]
[{"$nulls":3},"滑石笔",null,null,1]
[{"$nulls":3},"手套",null,null,25]
[{"$nulls":3},"扎丝","35mm长（包）",null,3]
[]
["合  计"]
["抹灰、镶贴工操作 实训室",null,100,"灰槽","2m*2m",null,1,{"$nulls":3},"抹灰、镶贴工操作实训室是对学生进行抹灰、镶贴施工工艺，方法的教学和学生进行相关技能训练的场所，要求学生掌握抹灰、镶贴常规工具的使用方法。帮助学生掌握最基本的抹灰、镶贴施工方法"]
[{"$nulls":3},"砂浆搅拌机","60L",null,2]
[{"$nulls":3},"双轮车",null,null,5]
[{"$nulls":3},"铁铲",null,null,50]
[{"$nulls":3},"砂浆桶",null,null,50]
[{"$nulls":3},"钢卷尺","5m",null,50]
[{"$nulls":3},"铝合金直尺","3m",null,50]
[{"$nulls":3},"靠尺","1m",null,50]
[{"$nulls":3},"托线板、线锤",null,null,50]
[{"$nulls":3},"铁抹子",null,null,50]
[{"$nulls":3},"塑料抹子",null,null,50]
[{"$nulls":3},"托灰板",null,null,50]
[{"$nulls":3},"阴角，阳角抹子",null,null,50]
[{"$nulls":3},"钢筋卡子","自制",null,50]
[{"$nulls":3},"小铁抹子",null,null,50]
[{"$nulls":3},"橡皮锤子",null,null,50]
[{"$nulls":3},"墨斗",null,null,50]
[{"$nulls":3},"瓷砖切割机","西德勒手动瓷砖切割机800手推式",null,10]
[{"$nulls":3},"空气压缩机","风豹空压机2524（780W）",null,1]
[{"$nulls":3},"激光水平仪","莱赛激光水平仪SP-L69IIS L69IIDS",null,5]
[]
["合计"]
["架子工操作实训室",null,150,"钢管","φ48、6米长",null,5,{"$nulls":3},"架子工操作实训室是对学生进行架子工教学及架子工技能训练的教学场所。通过实训使学生认识、掌握脚手架搭设材料、配件的种类及质量检验方法。通过实训使学生能搭设扣件式钢管脚手架"]
[{"$nulls":3},"对接扣件",null,null,300]
[{"$nulls":3},"十字扣件",null,null,400]
[{"$nulls":3},"旋转扣件",null,null,400]
[{"$nulls":3},"脚手板","0.8*2.2m",null,50]
[{"$nulls":3},"防护网","2000目/100平方厘米",null,50]
[{"$nulls":3},"门式脚手架",null,null,35]
[{"$nulls":3},"扳手","22号",null,35]
[{"$nulls":3},"钢尺","5M",null,35]
["合计"]
["总  计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}